# Washstand Clea-P made from the copolymer-bound mineral material VARICOR® (material in accordance to ISO norm 19712). Homogeneous, coloured throughout, pore-free material, without surface sealing like gel coat or glaze, largely resistant against disinfectants and commonly-used chemicals, heat resistant against burning cigarette, standard plain white colour shades (arktis, white-alpine) have good antibacterial properties in accordance to ISO 22196 (other colours on request). Optionally available with antiviral properties.

**Single washstand** moulded to order in one piece, m**ultiple washstand** made of several single washstands bonded together seamlessly and ready made-up, with side shelves, machinable on site, with integrated round countertop basin, without overflow, optional tap hole, with skirt, with chamfered wall-connection profile, with back rim for hanger bolt fastening. The permanent drain with VARICOR® cover is included in the scope of delivery.

**Clea-P** meets the requirements of the CE standard in compliance with DIN EN 14688.

Internal basin dimensions (L x W x D): Ø 360 x 140 mm

Depth: 550 mm

Material thickness: 12 mm

at the basin edge: 10 mm

Skirt: H = 150 mm

Chamfered wall-connection profile: H = 5 mm

Length of single washstand: 500 – 2500 mm

Length of multiple washstand: from 1000 mm

Attachment: Hanger bolts (included),

480-mm wall-mounting bracket for alcove installation   
(available as additional accessories)

Accessories (optional): • 480-mm wall-mounting bracket for alcove installation

Optional features: • Side section, seamlessly bonded left and/or right

• Functional cut-out (e.g. towel holder)

• Paper waste tube (round or rectangular), seamlessly   
 bonded

**Model: Clea-P**

**Distribution via: VARICOR GmbH**

**Waldstr. 33**

**76571 Gaggenau (Germany)**

**Tel.: +49 (0) 7225/9739-0**

[www.varicor.com](http://www.varicor.com)