# Washstand Jerico 550 made from the copolymer-bound mineral material VARICOR® (material in accordance to ISO norm 19712). Homogeneous, coloured throughout, pore-free material, without surface sealing like gel coat or glaze, largely resistant against disinfectants and commonly-used chemicals, heat resistant against burning cigarette, standard plain white colour shades (arktis, white-alpine) have good antibacterial properties in accordance to ISO 22196 (other colours on request). Optionally available with antiviral properties.

**Single washstand** moulded to order in one piece, **multiple washstand** made of several single washstands bonded together seamlessly and ready made-up, with side shelves, machinable on site, barrier free, with rectangular basin, standard without overflow, optional tap hole, with skirt, with flood rim along the front edge of the shelf, with chamfered wall-connection profile, with back rim for hanger bolt fastening.

**Jerico 550** qualifies for CE marking in compliance with DIN EN 14688 and meets the accessibility requirements according to DIN 18040.

Internal basin dimensions (L x W x D): 480 x 360 x 90 mm

Depth: 550 mm

Material thickness: 12 mm

Skirt: H = 50 mm

with flood rim H = 5 mm

Chamfered wall-connection profile: H = 40 mm

Length of single washstand: 650 – 1500 mm

Length of multiple washstand: from 1300 mm

Attachment: Hanger bolts (included)

 480-mm wall-mounting bracket for alcove installation

 (available as additional accessories)

Accessories (optional): • Permanent drain with VARICOR® cover

 (for basins without overflow)

 • 480-mm wall-mounting bracket for alcove installation

Optional features: • Side section, seamlessly bonded left and/or right

 • Paper waste tube (round or rectangular), seamlessly

 bonded

**Model: Jerico 550**

**Distribution via: VARICOR GmbH**

 **Waldstr. 33**

 **76571 Gaggenau (Germany)**

 **Tel.: +49 (0) 7225/9739-0**

[www.varicor.com](http://www.varicor.com)