# Washstand Agilo made from the copolymer-bound mineral material VARICOR® (material in accordance to ISO norm 19712). Homogeneous, coloured throughout, pore-free material, without surface sealing like gel coat or glaze, largely resistant against disinfectants and commonly-used chemicals, heat resistant against burning cigarette, standard plain white colour shades (arktis, white-alpine) have good antibacterial properties in accordance to ISO 22196 (other colours on request). Optionally available with antiviral properties.

**Single washstand** moulded to order in one piece, **multiple washstand** made of several single washstands bonded together seamlessly and ready made-up, with side shelves, machinable on site, barrier free, with projecting rectangular basin, material thickness in shelf area 20 mm, standard without overflow, optional tap hole, with skirt, with chamfered wall-connection profile, with back rim for hanger bolt fastening.

**Agilo** qualifies for CE marking in compliance with DIN EN 14688 and meets the accessibilityrequirementsaccording to DIN 18040.

Internal basin dimensions (L x W x D): 468 x 350 x 85 mm

Depth (centre of basin/shelf): 550 / 250 mm

Material thickness: 12 mm / 20 mm

Chamfered wall-connection profile: H = 10 mm

Length of single washstand: 800 – 2500 mm

Length of multiple washstand: from 1750 mm

Attachment: Hanger bolts (included)

180-mm wall-mounting bracket for alcove installation   
(available as additional accessories)

Accessories (optional): • Permanent drain with VARICOR® cover  
 (for basins without overflow)

• 180-mm wall-mounting bracket for alcove installation

Optional features: • Multifunctional cut-out left and/or right (grab handle)  
 245 x 60 mm

**Model: Agilo**

**Distribution via: VARICOR GmbH**

**Waldstr. 33**

**76571 Gaggenau (Germany)**

**Tel.: +49 (0) 7225/9739-0**

[www.varicor.com](http://www.varicor.com)