# Washstand Plano70-P made from the copolymer-bound mineral material VARICOR® (material in accordance to ISO norm 19712). Homogeneous, coloured throughout, pore-free material, without surface sealing like gel coat or glaze, largely resistant against disinfectants and commonly-used chemicals, heat resistant against burning cigarette, standard plain white colour shades (arktis, white-alpine) have good antibacterial properties in accordance to ISO 22196 (other colours on request). Optionally available with antiviral properties.

**Single washstand** moulded to order in one piece, **multiple washstand** made of several single washstands bonded together seamlessly and ready made-up, with side shelves, machinable on site, with rectangular basin, standard without overflow, optionally possible with external overflow, optional tap hole, with skirt, with chamfered wall-connection profile, with back rim for hanger bolt fastening,

**Plano70-P** meets the requirements of the CE standard in compliance with DIN EN 14688.

Internal basin dimensions (L x W x D): 700 x 310 x 105 mm

Depth: 500 mm

Material thickness: 12 mm

Skirt: H = 150 mm

Chamfered wall-connection profile: H = 5 mm

Length of single washstand: 800 – 2500 mm

Length of multiple washstand: from 1600 mm

Attachment: Hanger bolts (included)

 180-mm wall-mounting bracket for alcove installation

 (available as additional accessories)

Accessories (optional): • Permanent drain with VARICOR® cover

 (for basins withoutoverflow)

 • Push-open with VARICOR® cover

 (for basins with overflow)

 • 180 mm wall-mounting bracket for alcove installation

Optional features: • Side section, seamlessly bonded left and/or right

 • Functional cut-out (e.g. towel holder)

 • Paper waste tube (round or rectangular), seamlessly

 bonded

**Model: Plano70-P**

**Distribution via: VARICOR GmbH**

 **Waldstr. 33**

 **76571 Gaggenau (Germany)**

 **Tel.: +49 (0) 7225/9739-0**

[www.varicor.com](http://www.varicor.com)