# Washstand Privo made from the copolymer-bound mineral material VARICOR® (material in accordance to ISO norm 19712). Homogeneous, coloured throughout, pore-free material, without surface sealing like gel coat or glaze, largely resistant against disinfectants and commonly-used chemicals, heat resistant against burning cigarette, standard plain white colour shades (arktis, white-alpine) have good antibacterial properties in accordance to ISO 22196 (other colours on request). Optionally available with antiviral properties.

**Single washstand** moulded to order in one piece, **multiple washstand** made of several single washstands bonded together seamlessly and ready made-up, with side shelves, machinable on site, barrier free, in shelf area 20 mm, with projecting round basin, standard without overflow, optional tap hole, with skirt, with back rim for hanger bolt fastening.

**Privo** qualifies for CE marking in compliance with DIN EN 14688 and meets the accessibility requirements according to DIN 18040.

Internal basin dimensions (Ø x D): Ø 355 x 85 mm

Depth (centre of basin/shelf): 550 / 250 mm

Material thickness: 12 mm / 20 mm

Chamfered wall-connection profile: H = 10 mm

Length of single washstand: 700 – 2500 mm

Length of multiple washstand: from 1500 mm

Attachment: Hanger bolts (included)

 180-mm wall-mounting bracket for alcove installation

 (available as additional accessories)

Accessories (optional): • Permanent drain with VARICOR® cover

 (for basins without overflow)

 • 480-mm wall-mounting bracket for alcove installation

Optional features: • Multifunctional cut-out right and/or left (grab handle)
 200 x 40 mm

**Model: Privo**

**Distribution via: VARICOR GmbH**

 **Waldstr. 33**

 **76571 Gaggenau (Germany)**

 **Tel.: +49 (0) 7225/9739-0**

[www.varicor.com](http://www.varicor.com)