# Washstand Quebec-M made from the copolymer-bound mineral material VARICOR® (material in accordance to ISO norm 19712). Homogeneous, coloured throughout, pore-free material, without surface sealing like gel coat or glaze, largely resistant against disinfectants and commonly-used chemicals, heat resistant against burning cigarette, standard plain white colour shades (arktis, white-alpine) have good antibacterial properties in accordance to ISO 22196 (other colours on request). Optionally available with antiviral properties.

**Single washstand** moulded to order in one piece, **multiple washstand** made of several single washstands bonded together seamlessly and ready made-up, with side shelves, machinable on site, with rectangular basin with slot drain, standard without overflow, optionally possible with external overflow, optional tap hole, with skirt, with chamfered wall-connection profile, to be layed on a furniture or wall mounted.

**Quebec-M** qualifies for CE marking in compliance with DIN EN 14688.

Internal basin dimensions (L x W x D): 540 x 330 x 82 mm

Depth: 500 mm

Material thickness: 12 mm

Skirt: H = 50 mm

Chamfered wall-connection profile: H = 5 mm

Length of single washstand: 600 – 2500 mm

Length of multiple washstand: from 1200 mm

Attachment: To be layed on a furniture or wall mounted

For wall mounting: 407 mm angle bracket

480-mm wall-mounting bracket for alcove installation

(available as additional accessories)

Accessories (optional): • 407 mm angle bracket

• 480-mm wall-mounting bracket for alcove installation

• Connection piece for trap (included)

Optional features: • Side section, seamlessly bonded left and/or right

• Paper waste tube (round or rectangular), seamlessly

bonded

**Model: Quebec-M**

**Distribution via: VARICOR GmbH**

**Waldstr. 33**

**76571 Gaggenau (Germany)**

**Tel.: +49 (0) 7225/9739-0**

[www.varicor.com](http://www.varicor.com)