# Washstand Wetset made from the copolymer-bound mineral material VARICOR® (material in accordance to ISO norm 19712). Homogeneous, coloured throughout, pore-free material, without surface sealing like gel coat or glaze, largely resistant against disinfectants and commonly-used chemicals, heat resistant against burning cigarette, standard plain white colour shades (arktis, white-alpine) have good antibacterial properties in accordance to ISO 22196 (other colours on request). Optionally available with antiviral properties.

**Single washstand** moulded to order in one piece, **multiple washstand** made of several single washstands bonded together seamlessly and ready made-up, with side shelves, machinable on site, barrier free, with projecting round basin, standard with overflow, optional tap hole, with skirt, with chamfered wall-connection profile.

**Wetset** is barrier free qualifies for CE marking in compliance with DIN EN 14688.

Internal basin dimensions (Ø x D): Ø 400 x 192 mm

Depth (centre of basin/shelf): 570 / 340 mm

Material thickness: 12 mm

Skirt: H = 60 / 100 mm

Chamfered wall-connection profile: H = 20 mm

Length of single washstand: 750 – 2500 mm

Length of multiple washstand: ab 1650 mm

Attachment: Hanger bolts (included)

 180-mm wall-mounting bracket for alcove installation

 (available as additional accessories)

Accessories (optional): • Permanent drain with VARICOR® cover

 (for basins without overflow)

 • Push-open with VARICOR® cover

 (for basins with overflow)

 • 180-mm wall-mounting bracket for alcove installation

Optional features: • Side section, seamlessly bonded left and/or right

 • Basin facing

 • Paper waste tube (round or rectangular), seamlessly

 bonded

**Model: Wetset**

**Distribution via: VARICOR GmbH**

 **Waldstr. 33**

 **76571 Gaggenau (Germany)**

 **Tel.: +49 (0) 7225/9739-0**

[www.varicor.com](http://www.varicor.com)